 
 ------------------- SUMMARY -------------------
 
              ---------------------
        **** | INFORMATION SUMMARY | ****
              ---------------------
 
 The information obtained from the input file
 titled, "
 Shielding_Effectiveness_One_Click_blank.emin                                   
                                                      ", is summarized below:
              [All Units in MKSA]
 
 TIMESTEPS:
 
 The time increment             =   2.5499999E-12
 Number of specified time steps =                  10000
     The final simulation time =   2.5497449E-08
 
 
 
 SPACESTEPS:
 
 The origin is located at the cartesian coordinates:
 (x,y,z) = ( -0.1402080     , -0.1127760     , -1.0668000E-02 )
 
 The problem space indices span the following
 ranges:    X:            1    ->          185
            Y:            1    ->          149
            Z:            1    ->           65
 
 The mesh consists of:
 A constant x-increment of   1.5240000E-03
 A constant y-increment of   1.5240000E-03
 A constant z-increment of   1.5240000E-03
 
 
 
 BOUNDARY CONDITIONS:
 
 The following boundary conditions have been specified:
 
 All boundaries: PML                   
 
 The parameters of the perfectly matched layers
 (PML) boundary condition are:
   -                 The number of layers   =            8
   - The order of the conductivity function =    2.000000    
   -                 The percent reflection =   1.0000000E-03
 
 
 
 PLANE WAVE SOURCE:
 
 A plane wave source implemented with -
     a propagation vector polar angle of            1.570796    
     a propagation vector azimuthal angle of       0.0000000E+00
     an electric field vector polar angle of       0.0000000E+00
     an electric field vector azimuthal angle of   0.0000000E+00
 
     read in from file, "Plane_Wave.dat"
 
 The volume in which the plane wave source is
 implemented exist between the following finite
 difference grid indices:
         x-indices ->            4  to          182
         y-indices ->            4  to          146
         z-indices ->            4  to           62
 
 The plane wave originates in a region with the
 following electromagnetic parameter values:
             conductivity =   0.0000000E+00
             permittivity =   8.8540885E-12
             permeability =   1.2570126E-06
    magnetic conductivity =   0.0000000E+00
 
 
 
 MATERIALS:
 
 The following materials have been specified
 
       Material       | Number of | Number of | Number of | Number of |
         Type         |  Bodies   | Surfaces  |   Lines   |  Points   |
 ---------------------|-----------|-----------|-----------|-----------|
   Linear Background  |          1|     -     |     -     |     -     |
   Isotropic Nonmetal |          0|        228|          0|          0|
 
 Note: Background regions are tabulated under bodies.
 
 
 
 NEW PROBE:
 
 |           |         Number of probe points           |
 |           |------------------------------------------|
 | New Probe |      Numerical     ||       Prony        |
 |  Entity   |------------------------------------------|
 |           | Time | Freq | Tran || Time | Freq | Tran |
 |-----------|------------------------------------------|
 | Ex-Field  |   343|     0|     0||     0|     0|     0|
 | Ey-Field  |   343|     0|     0||     0|     0|     0|
 | Ez-Field  |   343|     0|     0||     0|     0|     0|
 
 
 
 APPROXIMATE MEMORY USAGE (MegaBytes):
 
 Field Quantities:                              86
 PML Boundaries:                               129
 
 ------------ End of Summary File ------------
 
